SECTION 08 42 33 – REVOLVING DOOR ENTRANCES

1. GENERAL
   * + 1. SUMMARY
          1. Section includes revolving door entrances.
          2. Related Requirements:

Section 03 3000 "Cast-in-Place Concrete" for block outs for recesses required for revolving door entrance. Section 05 50 00 "Metal Fabrications" for overhead supports that attach revolving door entrance framing to structure.

Section 08 41 13 "Aluminum-Framed Entrances and Storefronts" for adjacent aluminum entrance doors and storefront framing.

Section 08 44 13 "Glazed Aluminum Curtain Walls" for adjacent glazed aluminum curtain wall framing.

Section 08 88 00 "Glazing" for general requirements for installation of glass units in revolving door entrances.

Division 26 electrical power section for wiring requirements for revolving door entrances.

Section 28 13 00 "Access Control" for security access system providing control for door access and intrusion detection systems interfacing with revolving door entrance controls.

* + - 1. REFERENCE STANDARDS
         1. American Architectural Manufacturers Association (AAMA)

AAMA 611 Voluntary Specification for Anodized Architectural Aluminum

* + - * 1. American Association of Automatic Door Manufacturers (AAADM)

AAADM Certification Training Program

* + - * 1. ASTM International (ASTM)

ASTM A 36 / A36 Standard Specification for Carbon Structural Steel.

ASTM A 240 / A 240M Standard Specification for Chromium and Chromium-Nickel Stainless Steel Plate, Sheet, and Strip for Pressure Vessels and for General Applications

ASTM A 666 Standard Specification for Annealed or Cold-Worked Austenitic Stainless Steel Sheet, Strip, Plate, and Flat Bar

ASTM B 209 Standard Specification for Aluminum and Aluminum-Alloy Sheet and Plate.

ASTM B 221 / ASTM B 221M Standard Specification for Aluminum and Aluminum-Alloy Extruded Bars, Rods, Wire, Profiles, and Tubes

ASTM C 1048 Standard Specification for Heat-Strengthened and Fully Tempered Flat Glass

ASTM C 1172 Standard Specification for Laminated Architectural Flat Glass

ASTM E 283 Standard Test Method for Determining Rate of Air Leakage Through Exterior Windows, Curtain Walls, and Doors Under Specified Pressure Differences Across the Specimen.

ASTM E 330 Standard Test Method for Structural Performance of Exterior Windows, Doors, Skylights and Curtain Walls By Uniform Static Air Pressure Difference.

* + - * 1. Builders Hardware Manufacturers Association (BHMA)

BHMA A156.27 Power and Manual Operated Revolving Pedestrian Doors

* + - * 1. Code of Federal Regulations

16 CFR 1201 Safety Standard for Architectural Glazing Materials

* + - * 1. International Code Council (ICC)

ICC A117.1 Accessible and Usable Buildings and Facilities (ANSI)

* + - * 1. National Fire Protection Association (NFPA)

NFPA 70 National Electric Code.

NFPA 101 Life Safety Code.

* + - 1. ADMINISTRATION
         1. Coordination:

Recesses: Coordinate size and location of recesses in floor construction for revolving door entrance components including anchorages for frames and supports.

Anchorages: Furnish setting drawings, templates, and directions for installing anchorages that are to be embedded into concrete.

* + - * 1. Pre-installation Conference: Conduct conference at Project Site.
      1. ACTION SUBMITTALS
         1. Product Data: For each type of revolving door entrance specified.

Include details, material descriptions, dimensions and profiles, and finishes.

Include rated capacities, operating characteristics, electrical characteristics, and specialties and accessories.

* + - * 1. Shop Drawings: For revolving door entrances.

Include plans, elevations, sections, attachment details, dimensions, required clearances, methods of field assembly, and location and size of each field connection.

Indicate enclosures, speed control units, and components.

Indicate locations of activation and safety devices.

Include diagrams for power, signal, and control wiring.

* + - * 1. Samples for Verification: For each exposed component including hardware, for each color and finish selected, as required by architect.
      1. INFORMATIONAL SUBMITTALS
         1. Qualification Data: For qualified installer.
         2. Field quality control reports.
         3. Warranty: Sample of unexecuted manufacturer warranty.
         4. Manufacturers product information and applicable sustainability program credits that are available towards a LEED rated product certification.

Credit MR 4.1 and 4.2: Manufacture’s or fabricator’s certificate indicating percentage of post-consumer recycled content by weight and pre-consumer recycled content by weight for each product specified under this section.

* + - 1. CLOSEOUT SUBMITTALS
         1. Maintenance Data: For revolving door entrances, to include in operation and maintenance manuals.
      2. QUALITY ASSURANCE
         1. Installer Qualifications: Experienced Installer equipped and trained by manufacturer for installation and maintenance of units required for this Project, and who employs a Certified Inspector.
         2. Certified Inspector Qualifications: Certified by AAADM.
      3. DELIVERY, STORAGE, AND HANDLING
         1. Package revolving door entrance components individually with fasteners and installation templates; label and identify each package with door opening designation corresponding to Door Schedule.
         2. Store components in weather-protected area in manufacturer's unopened packaging until ready for installation.
         3. Protect materials from exposure to weather. Do not deliver until after wet work is complete.

Contact SPEC NOW for specific warranties on door construction.

* + - 1. WARRANTY
         1. Special Manufacturer's Warranty: Standard form in which manufacturer agrees to repair or replace components of revolving door entrances that demonstrate deterioration or faulty operation due to defects in materials or workmanship under normal use within warranty period specified.

Fabrication Warranty Period: Five (5), years from date of Substantial Completion.

Speed Control Ten (10) years from date of Substantial Completion.

Finish Warranty: Anodized Finish: Five (5) Years, Painted Finishes: Five (5) Years **[Ten (10) and Twenty (20) year finish Warranties Available]**

1. PRODUCTS
   * + 1. MANUFACTURERS
          1. Basis-of-Design Product: Provide revolving door entrances manufactured by Crane Revolving Door, dormakaba, Lake Bluff, IL; (844)-SPEC-NOW (844)773-2669; email: [**specnow.us@dormakaba.com**](mailto:specnow.us@dormakaba.com); website: [www.dormakaba.](http://www.dormakaba.)**us**

Choose the correct clause as required below select either “B” or “C”

* + - * 1. **[Substitutions: Requests for substitution and product approval in compliance with the specification must be submitted in writing and in accordance with the procedures outlined in Division 1, Section “Substitution Procedures”. Approval of requests is at the discretion of the architect, owner, and their designated consultants.]**
        2. **[Substitutions Not Permitted]**
        3. Source Limitations: Obtain revolving door entrance components through one source from a single manufacturer.
      1. PERFORMANCE REQUIREMENTS
         1. Performance Standard: Comply with ANSI A156.27.
         2. Opening Force, Maximum Turning Speed, Emergency Breakout, and Entrapment-Prevention Force: Comply with cited BHMA standard and requirements of authorities having jurisdiction.
         3. Safety Glass: Category II materials complying with testing requirements in 16 CFR 1201.
         4. Air Infiltration: Maximum air leakage through fixed glazing and framing areas of 1.25 cfm/sq. ft. (6.4 L/s x sq. m) of fixed entrance-system area when tested according to ASTM E 283 at a minimum static-air-pressure difference of 6.24 lbf/sq. ft. (300 Pa).
         5. Electrical Components, Devices, and Accessories: Listed and labeled as defined in NFPA 70 under UL 325.
      2. REVOLVING DOOR ENTRANCES
         1. Revolving Door Entrances with Breakout: Manufacturer's standard **[three-wing] [four-wing]** revolvingdoor entrances, including center shaft, speed control unit, wings, enclosure walls, canopy, glass and glazing, controls, hardware, and accessories as required for a complete and functional installation, of sizes and configuration indicated on Drawings.

Basis of Design: **dormakaba Crane 4000 Series**.

Unit Size and Attachment: As indicated on Drawings.

Manual Operation: Mechanical speed control unit (floor mounted), machined steel casting, with gear train, steel brake drum, and adjustable and replaceable brake blocks, adjustable to limit manually-applied speed of rotation overhead.

Pivot Bearing: Mounted opposite speed control allowing free rotation of center shaft.

Curved Enclosure Walls: Manufacturer's standard, with 1-3/4-inch- (45-mm-) thick tubular framing members.

Bookfold Mechanism Device: Emergency egress door leaves are configured with door hardware to permit collapse under adjustable pressure of 60 to 180 lbs. (265 to 800 N) applied to outer stile edge.

Chilled cast, precision machined bronze hangers and discs finished to match door. Adjustable spring tension set in field by installer to comply with applicable Life Safety and governing codes.

Mechanism: Wings are held in radial positions by means of steel balls, engaging in top and bottom disc of each wing. Excess pressure shall rotate balls from socket and allow each wing to be bookfolded. Tension shall be adjustable.

Center shaft shall be one-piece steel rod with aluminum housing to fit contour of wing, with felt seal mounted in wing stiles providing positive air lock at center of door.

Curved Enclosure Walls:

**[Formed Bronze] [Formed Stainless steel] [Extruded Aluminum]** Frames: Finish metal cut, formed and reinforced, and fitted over metal subframe fully welded with exposed finishes dressed after welding. Enclosure bases removable for field glazing.

Post and Base: Recessed below finished floor connected with steel mounting clips set in floor of finished concrete.

Curved Enclosure Glass Panels: 9/16” Clear laminated glass.

Select from item 9, 10 or 11 for the type of Door Wings and special sizing if required.

**Door Wings: Herculite** **[Formed Stainless Steel] [Formed Bronze] fully welded with exposed finishes dressed after welding to match enclosure frame. Herculite type 4-15/16” min. sight line.**

**Door Wings: Patch Fitting Extruded Aluminum cladded in [Formed Stainless Steel] [Formed Bronze] [Formed aluminum] custom cladded and finished in factory. Patch Fitting 6-1/16” sight line.**

**Door Wings: Cladded Herculite [Aluminum] [Formed Stainless Steel] [Formed Bronze] custom cladded and finished in factory. Herculite fitting 4-1/4” sight line.**

Bumper: Rubber tipped round button, two per wing installed on the push bar to separate door wings when bookfolded.

Weather Seals: Manufacturer's standard rubber and felt sweeps at wing lead edges and tops, and rubber at bottom.

Canopy, All Glass 13/16” clear polyurethane laminated glass with exposed and polished edges. (See drawings for configuration of glass canopy.)

Locks: Mortised deadbolt locks, one each concealed in two adjacent bottom rails for interior locking into floor, with two mounted dustproof strikes.

Choose from item “a” to “d”. Custom push bars available. Contact SPEC Now for additional information.

* + - * 1. **Push Bars:**

**1” Diameter Horizontal Push Bar (matching wing)**

**1” Diameter Vertically Mounted Push Bar (matching wing)**

**Decorative Push Bar: As selected by Architect from manufacturer's full line.**

* + - 1. ACCESSORIES
         1. **[Welded Floor Grilles: Concentrically Curved quarter quadrant (90 degree section) radius Grilles fabricated from concentrically rolled circles of stainless steel are to be welded and formed from type 304 stainless steel ¼” x 1” solid bars and polished to a Satin finish. Complete with recessed floor pan welded from 12-gauge stainless steel with an available drainage fitting. (see drawing for details.]**

Contact SPEC NOW for more information on Access Control

* + - * 1. **[Access Control Actuation: revolving door actuation by external card reader, biometric reader, key pad or remote push button. Actuation devices provided by not limited to dormakaba.]**
        2. **[Self positioning closer (Return to home), automatically resets the door to its home (X) position after every use to provide an optimal weather seal while door is idle. Minimum canopy height of 6 1/2” required. uses 120VAC.] Return to Quarter Point is required for the S1 security feature.**
        3. **[Security S1 Locking device with automatic shutter bolt and wing lock with return to quarter point with self-positioning closer. Remote switch capable.]**
      1. MATERIALS
         1. Aluminum Extrusions: ASTM B 221; 6063 alloy, T5 temper, 0.125 inch (3 mm) minimum thickness except stops and canopy covers 0.0625 inch (1.58 mm).
         2. Aluminum Sheet: ASTM B 209; 5005 alloy, H15 or H34 temper, 0.080 inch (2 mm) minimum thickness.
         3. Stainless Steel: ASTM A 240/A 240M; Type 304 rollable temper, 0.060 inch (1.5 mm) minimum thickness minimum thickness.
         4. Bronze Extrusions: ASTM B 455, architectural bronze alloy **[No. 220 Commercial] [No. 280 Muntz] [nickel silver]**, 0.125 inch (3 mm) minimum thickness.
         5. Steel Sections: ASTM A 36; shapes to suit mullion sections, galvanized.
         6. Sheet Steel: ASTM A 653/A 653M; galvanized to G90 (Z275), 0.106 inch (2.6 mm) minimum thickness.
         7. Fasteners and Accessories: Corrosion-resistant, nonstaining, nonbleeding fasteners and accessories compatible with adjacent materials.
         8. Glass Panels, General: Provide glass panels that comply with 16 CFR 1201, Category II requirements for safety glazing. Permanently mark glazing with certification label of the SGCC. All glass shall meet ANSI standard Z 97.1

Enclosure Curved Glass Panels: Clear Laminated glass 9/16” (14.28mm).

Framed Wing Glass Panels: Clear Tempered glass ½” (12.7mm).

Canopy Glass:13/16” clear polyurethane laminated glass.

Tint Color: [As selected by Architect from manufacturer's full line]

* + - 1. **FINISHES**

Contact SPEC Now for custom finish options. Choose type of finish and type color and/or metal.

* + - * 1. Comply with NAAMMs “Metal Finishes Manual for Architectural and Metal Products” for recommendations for applying and designating finishes.
        2. Rotating and Curved Enclosures: ***(Typically, same finish on both enclosures)***

Anodized Aluminum Finishes:

Clear AA M12C22A41 Anodized Class 1

**[Dark] [Medium] [Light] Bronze, [Black] [Champagne**] AA M12C22A44 Class1

Custom Anodized Finish as selected by architect.

Painted Finish:

**[Powder coat painted to match architects sample.]**

**[Kynar finish, [2 coat] [3 coat], to match architects sample.**

Clad Finish: Cladding shall be factory finished at manufacturers facility using .36 thick metalcladding panel surface utilizing tesa® 4965 tape. Heat and humidity resistant, the specialized adhesive tape is comprised of a polyester backing coated on both sides with a transparent modified acrylic adhesive and a tensile strength of 20 N/cm. tesa® 4965 is recognized per UL standard 969. UL file: MH 18055.

**[Stainless Steel #4 Satin]**

**[Stainless Steel #6 Satin]**

**[Stainless Steel #7 Mirror Polished]**

**[Custom Stainless as selected by the architect.]**

**[bronze #4Satin]**

**[bronze #6 Satin]**

**[bronze #7 Mirror Polished]**

**[US10B statuary finish]**

**[Special Bronze as selected by the architect]**

**Over 60+ configurations and variations in design to choose from. Please contact SPEC NOW For more information.**

1. EXECUTION
   * + 1. EXAMINATION
          1. Examine revolving door entrance opening to determine if work is within revolving door entrance manufacturer's required tolerances and ready to receive work.

Verify electrical power and control connections are properly located and of correct characteristics.

Verify recesses and supplemental framing comply with requirements on approved shop drawings.

* + - * 1. Proceed with installation once conditions affecting installation and performance of revolving door entrance meet manufacturer's requirements.
      1. REVOLVING DOOR ENTRANCE INSTALLATION
         1. General: Comply with revolving door entrance manufacturer's written installation instructions and approved shop drawings.
         2. Install revolving door entrances after other finishing operations have been completed.
         3. Set units level, plumb, and true to line, with uniform joints. Maintain assembly dimensional tolerances, aligning with adjacent Work.
         4. Secure revolving door entrance components to building structure and supports as indicated on approved shop drawings, utilizing approved fasteners and spacing.
         5. Install glass and enclosure panels in accordance with Section 088000 "Glazing."
         6. Install perimeter type sealant, backing materials, and to installation requirements in accordance with Section 079200 "Joint Sealants."
         7. Complete connections to electrical power, lighting, and controls in accordance with requirements of respective Division 26 and Division 28 Sections.
         8. Install wings, with operators and controls. Fit, align, and adjust assembly for smooth operation.
      2. ADJUSTING
         1. Adjust operating components and hardware to produce smooth operation and tight, uniform fit.
         2. Adjust revolving door entrances to required timing and force.
         3. Adjust latches and locks for smooth operation.
         4. Test and adjust components linked to access control system.
         5. Replace damaged components and accessories.
      3. CLEANING
         1. Clean finished surfaces in accordance with manufacturer's written instructions. Do not use cleaning agents or methods not approved by manufacturer.
         2. Clean exposed metal surfaces to factory new appearance.

END OF SECTION 084233